

|  |  |
| --- | --- |
| **Model:** | **Renova Nr. 1 Comfort Wash-down WC, without flushing rim 4,5/6 l, wall-hung 700 mm projection** |
| **Model No.** | **208570** |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

**Washdown WC, 4.5/6l**

**Rimless**

**CE, EN 997 - CL1 5A + 6AC, EN33**

**Wall-hung with 70 cm projection**

**Made of sanitary ware porcelain**

**CE-marked**

**For in-wall cabinet**

**DIN 18040**

**Particularly suitable for use by wheelchair users.**

**Brand:** KERAMAG

**Model:** Renova Nr. 1

**Model no.:** 208570

**Size:** Width: 350 mm, Depth: 700 mm

**Fastening:** Threaded rods M 12

**Outlet:** horizontal

**Optional:**

With permanently fired KeraTect(r) glaze, free of pores, surface roughness value in accordance with DIN 4768-ISO 4287 Ra < 0.01 µm (Colour code 600)

**Can be combined with:**

WC seat with continuous stainless steel hinge shaft 578510